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	assessment summary & record 



	activity
	METHOD
	desired outcomes 
	result

	NATURE OF ACTIVITY
	WRITTEN
	oral
	Portfolio
	OBSERVATION
	desired outcomes for successful assessment of competency standard:  Mason
	competent
	not yet competent

	Practical Skill Demonstration
	
	
	
	
	· Perform layout according to drawings/instructions
· Lay bricks/blocks according to instruction/ drawings
· Carryout concrete work according to instruction/ drawings
· Carryout Plaster and pointing according to instruction/ drawings
· Lay drains


	
	

	Knowledge Assessment	
	
	
	
	
	· Answer all questions your Assessor may have during the practical assessment.

	
	

	Other Requirements
	
	
	
	
	· N.A
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	 candidate assessment

	Candidate's Name………………………………………………..... Father’s Name …………………………………………………………………..

	

	all work assessed in this COMPETENCY STANDARD must be your own work.



	GUIDANCE TO CANDIDATE

	To meet this standard you are required to complete the following tasks within five hours timeframe:
· Construct a brick masonry wall size 4’ x9’’ x1’ for open drain of size 4.0’x1.0’x1.0’ with cement sand ratio (1:6), PCC base (1:4:8) of thickness 3’’ and plaster the walls  of the drain with cement mortar (1:6).Thickness of plaster is 3/4”    

· Pointing of brick wall panel 2’x2’ with cement sand ratio 1:2 





	ACTIVITies
	candidate response

	1. Complete practical task of “Mason” under observation by an assessor
	During a practical assessment, under observation by an assessor, I will correctly :

· Construct a brick masonry walls of size 4’x0.75’x1’ for open drain of size 4.0’x1.0’x1.0’ with cement sand ratio (1:6), horizontal mortar layer of ½ inch. PCC base (1:4:8) of thickness 3’’and plaster the walls of the drain with cement mortar (1:6).Thickness of plaster is ¾ ”   
· Draw a centre line of length 4’ with reference to given start point to perform a Layout of open drain of size 4.0’x1.0’x1.0’ 
· Draw offset lines on either side of the centre line at distance of 1.125’ from the centre line.
· If the mixing process done by the labour of cement, sand and crush is according to the ratio of 1:4:8.
· Fix  the formwork done by the labour is according to the size of base of open drain(4’x2.5’x0.25’)
· Lay down the P.C.C (1:4:8) at the specified site according to the size of base of open drain(4’x2.5’x0.25’)
· Compact the P.C.C with tamping rod of 5/8” diameter 
· Finish the P.C.C concrete surface with wooden float.
· Prepare cement mortar according to ratio (1:6) for the construction of masonry wall 4’x9’’x1’of an open drain 4.0’x1.0’x1.0’.
· Soak the brick if required. 
· Lay cement mortar of thickness 0.5 inch for the construction of a wall (4’X9’’ X 1’) of open drain on both sides.
· Lay bricks in layers by using English bond to construct a wall 4’X 9’’ X 1’
· Maintain vertical alignment of wall size 4’x9’’x1’ by using plumb bob
· Maintain horizontal alignment of wall size 4x9’’x1’ by using string and pins
· Finnish the surface of walls to remove extra mortar by using wire brush
· Apply cement slurry on brick wall panel to ensure adhesion of mortar with brick wall.
· Apply cement mortar ¾ inch thick on brick walls of size   open drain and level it with the help of trowel/straighter
· Finish the surface of wall 4x1’by using float.
· Adapt the safety measures as per work requirement.

· Pointing of brick wall panel 2’x2’ with cement sand ratio 1:2 
· If the brick wall panel 2’x2’ is cured.
· Set  the mixing process done by the labour of cement and sand is according to the ratio of 1:2
· Align the grooves of brick wall by using chisel to prepare the surface for pointing of brick wall panel 2’x2’
· Fill the gaps of joints of brick layers wall panel 2’x2’ by using cement sand mortar (1:2)
· Remove the excess mortar with the help of wire brush and leave a face joint that is just lower than the face of the wall.

· Important Note: The following general performance criteria will be followed and performed in all the tasks (where applicable) by the candidate in order to meet this standard.

1. Follow health and safety procedure as per the requirements of given task
1. Prepare work station as per the requirements of task
1. Select tools/ equipment as per the requirements of task
1. Report to supervisor in case of any contingency after taking necessary actions
1. Complete the work by following sequence of operations
1.    Perform task(s) within standard timeframe




	2. Other requirements
	· [N/A]

	3. Answer any questions your assessor may have during the practical assessment
	My answers to questions are correct and demonstrate my understanding of the topics and their application.
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	assessor judgement guide

	

	Candidate’s Name …………………………………………………   Father’s Name.……………………………………………………..

	INSTRUCTIONS FOR ASSESSOR 
	This section contains minimum evidence requirements. Oral questioning may be used to clarify candidate understanding of the topic and its application.



	Activities
	minimum evidence required 
	Yes
	No
	assessor comments

	1. Complete practical task of Mason under observation by an assessor
	During a practical assessment, under observation by an assessor, the candidate correctly carried out the following tasks:





	
	
	

	Construct a brick masonry walls of size 4’x0.75’x1’ for open drain of size 4.0’x1.0’x1.0’ with cement sand ratio (1:6), PCC base (1:4:8) of thickness 3’’and plaster the walls of the drain with cement mortar (1:6).Thickness of plaster is ¾ ”   

	Drawn a centre line of length 4’ with reference to given start point to perform a Layout of open drain of size 4.0’x1.0’x1.0’.
	
	
	

	
	Drawn offset lines on either side of the centre line at distance of 1.125’ from the centre line.

	
	
	

	
	Did the mixing process done by the labour of cement, sand and crush is according to the ratio of 1:4:8.
	
	
	

	
	Ensured whether the formwork done by the labour is according to the size of base of open drain (4’x2.5’x0.25’).

	
	
	

	
	Laid the P.C.C (1:4:8) at the specified site according to the size of base of open drain (4’x2.5’x0.25’).

	
	
	

	
	Compact the P.C.C with tamping rod of 5/8” diameter.

	
	
	

	
	Finished the P.C.C concrete surface with wooden float.

	
	
	

	
	Prepared a cement mortar according to ratio (1:6) for the construction of masonry wall 4’x0.75’x1’of an open drain 4.0’x1.0’x1.0’.

	
	
	

	
	Soaked the brick if required 
	
	
	

	
	Laid cement mortar of thickness 0.5 inch for the construction of a wall (4’X 0.75’ X 1’) of open drain both sides.
	
	
	

	
	Laid bricks in layers by using English bond to construct a wall 4’X 0.75’ X 1’.
	
	
	

	
	Checked vertical alignment of wall size 4’x9’’x1’ by using plumb bob
	
	
	

	
	Checked  horizontal alignment of wall size 4x9’’x1’ by using string and pins
	
	
	

	
	Finished the surface of walls to remove extra mortar by using wire brush.
	
	
	

	
	Applied cement slurry on brick wall panel to ensure adhesion of mortar with brick wall.
	
	
	

	
	Applied cement mortar ¾ inch thick on brick walls of open drain and level it with the help of trowel.
	
	
	

	
	Finished the surface of plaster by using float
	
	
	

	
	Adapted the safety measures as per work requirement.
	
	
	

	Pointing of brick wall panel 2’x2’ with cement sand ratio 1:2 

	Cured the brick wall panel 2’x2’ is.
	
	
	


	
	Did the mixing process done by the labour of cement and sand is according to the ratio of 1:2.
	
	
	

	
	Aligned the grooves of brick wall by using chisel to prepare the surface for pointing of brick wall panel 2’x2’.
	
	
	

	
	Filled the courses of brick wall panel 2’x2’ by using cement sand mortar (1:2).
	
	
	

	
	Removed the excess mortar with the help of wire brush and leave a face joint that is just lower than the face of the wall.
	
	
	

	General performance criteria
	Follow health and safety procedure as per the requirements of given task
	
	
	


	
	Prepare work station as per the requirements of task
	
	
	

	
	Select tools/ equipment as per the requirements of task
	
	
	

	
	Report to supervisor in case of any contingency after taking necessary actions
	
	
	

	
	Complete the work by following sequence of operations perform task(s) within standard timeframe
	
	
	





















	3. Answer any questions the assessor may have during the practical assessment
	Candidate’s answers to questions are correct and demonstrate understanding of the topics and their application.

Assessor to document below all questions asked and candidate answers. Use extra sheets if required and attach.
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	List of TOOLS, equipment, material and context of assessment



	INSTRUCTIONS
	This section contains information regarding;

· Context of the assessment 
· List of required tools and equipment.
· List of consumable items required during the service

	1. Context of Assessment 
	This task will be performed in real time/simulated environment.



	2. List of tools and equipment required (for five candidates)

	S. No 
	Items
	Quantity

	1
	Trowel 
	05

	2
	Brick Hammer 
	05

	3
	Spirit Level
	05

	4
	String (length= 10 m)
	05

	5
	Pins 
	20

	6
	Straight Edge
	05

	7
	Plumb Bob
	05

	8
	Mason Square
	05

	9
	Steel tape 
	05

	10
	Hammer 
	05

	11
	Chisel
	05

	12
	Wheel Barrow 
	05

	13
	Wooden float
	05

	14
	Gloves 
	10

	15
	Shovel
	05

	16
	Steel Pan
	10

	17
	Wire Brush
	05

	18
	Safety Helmet
	05




	3. List of consumable items required (for five candidates)

	S. No 
	Items 
	Quantity

	1
	Cement
	350 Kg

	2
	sand
	2000 Kg

	3
	Crush
	600 Kg

	4
	bricks
	500 No

	5
	Lime powder
	25 Kg
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