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	assessment summary & record 



	activity
	METHOD
	desired outcomes 
	result

	NATURE OF ACTIVITY
	WRITTEN
	oral
	Portfolio
	OBSERVATION
	desired outcomes for successful assessment of competency standard: Mason
	competent
	not yet competent

	Practical Skill Demonstration
	
	
	
	
	· Perform stone work according to instructions/drawing and specification.
· Erect scaffolding according to instructions/drawing
· Fix doors and windows according to instructions/ drawing
· Carry out tiling work according to instructions/drawings

	
	

	Knowledge Assessment	
	
	
	
	
	· Answer all questions your Assessor may have during the practical assessment.

	
	

	Other Requirements
	
	
	
	
	· N.A
	
	





	2
	 candidate assessment

	Candidate's Name………………………………………………..... Father’s Name …………………………………………………………………..

	

	all work assessed in this COMPETENCY STANDARD must be your own work.



	GUIDANCE TO CANDIDATE

	To meet this standard you are required to complete the following tasks within Five hours  timeframe:
· Construct stone wall of size 4’x4’ of 13” thickness with cement mortar at ratio 1:6 at site.
· Carry out tiling work on the surface of 3’x3’ wall with tile size 1’x1’ with bond.
· Develop a platform of size 6’x2’x4’ by using scaffolding for fixing of window frame at a height 7’ from ground level. The size of the window is 3’x3’.




	ACTIVITies
	candidate response

	1. Complete practical task of “Mason” under observation by an assessor
	During a practical assessment, under observation by an assessor, I will correctly :

· Construct stone wall of size 4’x4’ of 13” thickness with cement mortar at ratio 1:6 at site.
· Carry out dressing of stone to make them uniform size.
· Confirm whether the mixing process done by the labour of cement and sand is according to the ratio of 1:6.
· Lay cement sand mortar on the bed of stone wall with thickness of 5 cm.
· Align the stone on the cement sand mortar layer to construct stone wall of size 4’x4’ of 13” thickness.
· Lay the second layer of stone to ensure that vertical joints are staggered.
· Maintain vertical alignment of wall by using plumb bob.
· Fill the joints in the wall with small pieces of stones.
· Fill the grooves by grouting the cement sand mortar (1:6) to strengthen it.
· Carry out tiling work on the surface of 3’x3’ wall with tile size 1’x1’ with bond

· Ensure the levels of the surface of 3’x3’ wall with hand level.
· Prepare the surface of the wall 3’x3’ with steel wire brush  
· Chip the surface of the wall to make bond of tile with wall.
· Prepare adhesive to be used within 30 minutes
· Apply adhesive of 1/4” on the surface of the tile and place it at desired location 
· Lay down tiles starting from the centre of the wall 3’x3’ by using tile spacer for uniform joints and to avoid sliding
· Tap in all tiles with a rubber hammer to ensure solid bond and level plane.
· Fill the grooves and joints of the tiles on the surface of wall 3’x3’ with a grout after getting some strength.
· Remove the excess grout by using damp sponge.
· Finish the surface and joints of tiles.
· Develop a platform of size 6’x2’x4’ by using scaffolding for fixing of window frame at a height 7’ from ground level. The size of the window is 3’x3’
· Fix vertical poles at required position with cross couplers / knots.
· Fix horizontal poles with couplers/knots.
· Lay the planks on horizontal poles to make temporary working platform.
· Attach the guardrails to avoid risk of fall.
· Inspect thoroughly the scaffolding to ensure safety.
· Prepare opening size for window frame of size 3’x3’ in the wall at a height 7’ from the ground. 
· Fix the hinges of the frame with the help of PCC (1:2:4) to fix window frame of size 3’x3’ in the wall at a height 7’ from the ground.
· Position the horizontal and vertical alignment of the window frames after completion of concreting operation. 
· Finnish the frame hinge area by using cement mortar (1:6).
· Adapt the safety measures as per work requirement.

·  Important Note: The following general performance criteria will be followed and performed in all the tasks (where applicable) by the candidate in order to meet this standard.

1. Follow health and safety procedure as per the requirements of given task
1. Prepare work station as per the requirements of task
1. Select tools/ equipment as per the requirements of task
1. Report to supervisor in case of any contingency after taking necessary actions
1. Complete the work by following sequence of operations
             Perform task(s) within standard timeframe
· 


	2. Other requirements
	· [N.A]

	3. Answer any questions your assessor may have during the practical assessment
	My answers to questions are correct and demonstrate my understanding of the topics and their application.




































	3
	assessor judgement guide

	

	Candidate’s Name …………………………………………………   Father’s Name.……………………………………………………..

	INSTRUCTIONS FOR ASSESSOR 
	This section contains minimum evidence requirements. Oral questioning may be used to clarify candidate understanding of the topic and its application.



	Activities
	minimum evidence required 
	Yes
	No
	assessor comments

	1. Complete practical task of Mason under observation by an assessor
	During a practical assessment, under observation by an assessor, the candidate correctly carried out the following tasks:





	
	
	

	Construct stone wall of size 4’x4’ of 13” thickness with cement mortar at ratio 1:6 at site.

	Carried out dressing of stone to make them same height and of 13” thickness.
	
	
	

	
	Confirmed whether the mixing process done by the labour of cement and sand is according to the ratio of 1:6.
	
	
	

	
	Laid cement sand mortar on the bed of stone wall with thickness of 5 cm.
	
	
	

	
	Aligned the stone on the cement sand mortar layer to construct stone wall of size 4’x4’ of 13” thickness.
	
	
	

	
	Laid the second layer of stone to ensure that vertical joints are staggered.
	
	
	

	
	Checked vertical alignment of wall by using plumb bob.

	
	
	

	
	Filled the joints in the wall with small pieces of stones.

	
	
	

	
	Filled the grooves by grouting the cement sand mortar (1:6) to strengthen it.

	
	
	

	Carry out tiling work on the surface of 3’x3’ wall with tile size 1’x1’ with bond

	Ensured the levels of the surface of 3’x3’ wall with hand level.
	
	
	

	
	Prepared the surface of the wall 3’x3’ with steel wire brush. 
	
	
	

	
	Chipped the surface of the wall to make bond of tile with wall
	
	
	

	
	Prepared adhesive to be used within 30 minutes.
	
	
	

	
	Applied adhesive of 1/4” on the surface of the tile and place it at desired location. 
	
	
	

	
	Laid tiles starting from the centre of the wall 3’x3’ by using tile spacer for uniform joints and to avoid sliding.
	
	
	

	
	Tapped in all tiles with a rubber hammer to ensure solid bond and level plane.
	
	
	

	
	Filled the grooves and joints of the tiles on the surface of wall 3’x3’ with a grout after getting some strength.
	
	
	

	
	Removed the excess grout by using damp sponge.
	
	
	

	
	Finished the surface and joints of tiles.
	
	
	

	Develop a platform of size 6’x2’x4’ by using scaffolding for fixing of window frame at a height 7’ from ground level. The size of the window is 3’x3’.

	Fixed vertical poles at required position with cross couplers / knots.
	
	
	

	
	Fixed horizontal poles with couplers/knots.
	
	
	

	
	Laid the planks on horizontal poles to make temporary working platform.
	
	
	

	
	Attached the guardrails to avoid risk of fall.
	
	
	

	
	Inspected thoroughly the scaffolding to ensure safety.
	
	
	

	
	Prepared opening size for window frame of size 3’x3’ in the wall at a height 7’ from the ground. 
	
	
	

	
	Fixed the hinges of the frame with the help of PCC (1:2:4) to fix window frame of size 3’x3’ in the wall at a height 7’ from the ground.
	
	
	

	
	Positioned the horizontal and vertical alignment of the window frames after completion of concreting operation. 
	
	
	

	
	Finished the frame hinge area by using cement mortar (1:6).
	
	
	

	
	Adapted safety measures as per work requirement.

	
	
	

	General Performance Criteria 


	Follow health and safety procedure as per the requirements of given task
	
	
	

	
	Prepare work station as per the requirements of task
	
	
	

	
	Select tools/ equipment as per the requirements of task
	
	
	

	
	Report to supervisor in case of any contingency after taking necessary actions
	
	
	

	
	Complete the work by following sequence of operations perform task(s) within standard timeframe
	
	
	

	2. Other requirements

	N/A
	
	
	
















	3. Answer any questions the assessor may have during the practical assessment
	Candidate’s answers to questions are correct and demonstrate understanding of the topics and their application.

Assessor to document below all questions asked and candidate answers. Use extra sheets if required and attach.
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	List of TOOLS, equipment, material and context of assessment



	INSTRUCTIONS
	This section contains information regarding;

· Context of the assessment 
· List of required tools and equipment.
· List of consumable items required during the service

	1. Context of Assessment 
	This task will be performed in real time/simulated environment.



	2. List of tools and equipment required (for five candidates)

	S. No 
	Items
	Quantity

	1
	Trowel 
	05

	2
	Tile Cutter 
	05

	3
	Spirit Level
	05

	4
	String (length= 10 m)
	05

	5
	Pins 
	20

	6
	Straight Edge
	05

	7
	Plumb Bob
	05

	8
	Mason Square
	05

	9
	Steel tape 
	05

	10
	Steel Pan
	05

	11
	Spacer
	100

	12
	Wheel Barrow 
	05

	13
	Shovel
	05

	14
	Wire Brush
	10

	15
	Stone Hammer
	05

	16
	Sponge 
	05

	17
	Scaffolding Key set
	05

	18
	Adjustable Screw wrench
	05

	19
	Cleaning cloth (length 1m)
	05

	20
	Safety Helmet
	05

	21
	Safety Shoes
	10

	22
	Safety Goggles
	05




	3. List of consumable items required (for five candidates)

	S. No 
	Items 
	Quantity

	1
	Tiles 1’x1’ 
	45 Sft

	2
	Tile Bond 
	5 Bags

	3
	Tile Bond
	5 Boxes

	4
	Stone 
	125 Cft

	5
	Cement
	50 kg

	6
	Sand
	300kg

	7
	MS Pipe (Length = 15’)
	20 No

	8
	MS Pipe (length= 10’)
	20 No

	9
	MS Joints 
	50 No

	10
	Window Frame (3’x3’)
	5 No

	11
	Wooden Planks (10’x1’x 1.125”)
	15
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